**Instructions for Loading/unloading the Roma box**

**DO NOT OPEN THE BOX** before reading these instructions.

**DO NOT** open the box on any other side other than the “Open **FRONT PANEL** only”

Move the box to a flat horizontal surface.

Lock at least 2 of the 4 wheels

Release the two Screws “A” and let the locking bar hang down.

Release both “Wings” by removing the two screws “B” from each “Wing”.

Place the locking bar into the central hole on the black bracket on the stabilising “Wing”.

Once both the “Wings” are secured in position the “Front Panel” can be removed.

Do not move the box with the “Wings” extended and touching the floor.

The load must be placed closer to the “Front Panel” to ensure stability during manipulation with the fork lift or transpalette.

http://rpc-cms-re4-upscope.web.cern.ch/rpc-cms-re4-upscope/RPC/Chamber%20Institutes/Shipping/Packing/RomaBox/Instructions for Loading.docx