***Up date on Infrstructure for GIF++***

***Cabling work last week***

All DCS have connectors meaning both Preparation and upstream are operational (HV,LV,DCS and signal) in terms of cables. Gas inspection this week

***Additional cables***

Current measurement for 10 chambers

Power for XY tables (s)

Camera video and power for X-Y table

Gas kill cable. Path, length, supply and installation

**Down Stream**

HV cable umbilical to move from 610.

DCS

LV

Signal cables

Cable to control room ?

HV cables for Scintillators

Signal cables for PMT.

***Infrastructure***

Move cable tray and cables from D\_Stream to U-Stream. Planned fro Thursday.

X-Y tables (Cosmic stand) and R&D

Long Term table ONLY 4 chambers at beam height.

**Safety**

ISIEC the old version not accepted. New one sent Monday 23 March 2015

Inspection with Bruno Plicher.

 Ian Crotty 21 March 2015