ENCV Room very small water leak under Bus bar circuit, photo.

Outside ENCV room sand to pick up oil ?, as reported before, but with what appears to be water on the green beam above, photos. Does not appear to change much.

It is dry in the USC -2 to -5deg C DP.

USC racks;

S2B17 rack on but no PC on.

S2F19 ditto

S2G02 Green light on rack turbine is off but the contents are on.

Surface.

B. 3584 Door not locked

Membrane plant .

On the screen of the installation nearest the entry door there is not the values screen as shown in the instructions but a schematic of the installation, photo.

Unable to toggle back to the screen shown. Called 165503 and identified similar values to those required BUT this is not a sufficient correlation.

Photos are here;

https://rpc-cms-re4-upscope.web.cern.ch/RPC/Safety/ActivityCavern/XmasSafetyTour2021to2022/

Many thanks Attila