Shelving in 904.

Orange and Blue shelving (Nominally for Palettes)

Shelves are 2680mm x 1110mm there are 8 levels (shelves) that are not equipped with shelving surfaces. We should find more bars for supporting shelving as they are at present spaced 105cm in height. Four more would be a reasonable number.

Wood from CERN stores

43 77 60 227.2 250mm x 27mm rough sawn timber 11chf/m2

43 79 30 222.2 1845mm x 5200mm x 22mm blockboard 35.5ch/m2

43 75 70 260.8 24mm x 600mm x 5000mm smooth timber 24.5chf/m2

Take care of the sense of the wood grain.

Old stored wood in 904 from packing cases.

Nominal calculation of surface area required = 8 x 2.68m x 1.11m = 24m2

Assuming zero lose cost Blockboard = 852chf

Smooth plancks = 588chf

Rough planks = 264chf

Add 200chf for screws and stabilising batterns .