Wooden Gap support Gas schematics #2

Top gap 1, 3, 5, 7

Bottom gap 2, 4, 6, 8

HV

 Connections are as for RE, namely Bottom is the central electrode

Top Gap circuit is

Bottom gap Circuit is 2 supply and 6 return

HV bot

HV top

2 1

3 4

8 7

6 5

1,2

3,4

7,8

5,6

Bottom gap next to thick panel

Top gap circuit is 7 supply and 3 return

 Ian Crotty 12 Nov 2010