Kiddi Nozzle from P5 Foam Installation

Internal dia XXmm

Inside is a mixer/Swirl

¾” BSP

L=16mm

Dia. 14.5mm

Nozzle int. dia 5.65mm

13.4mm

Material . Brass

Ian Crotty Nov 2013

AF24mm

68.05mm

12mm

Dia. 27mm