Foam test with one Nozzle

β

Foam Mixer

ZumiScher AWG

Water from Hydrant

Pressure gauge

P1

Flow measurement

Support palette type L=3m

Flow measurement

Foam Agent inlet

Ian Crotty

Feb 2014

Kiddi Nozzle

Holed plate

Hole dia 3.xxmm

Spacing XXXmm

Β = angle of incidence

Pressure gauge

P2

P1

Initial Version, Next version with pressure fed Foam Agent