Elog for 1 oct 2020

Replaced white mouse with old one from magnet, as it does not work easily.

0907hrs. Access control team (x2) Serge Di Luca, 164000, will be breaking tags on access doors in CMS/LHC.

0910hrs. Called 162680 for numerous GEM DCS alerts.

The charger connectors on the DCS station are not the same as on the shift leader desk, which mate solidly.

The phones (Cat B30) have "micro b USB" 5 pins. These are NOT symmetrical.

The DCS charging station lines , x5, seem to be something like "micro A USB" that are symmetrical.

These differences may well explain the poor charging of the DCS phones, connector is not locked in in a solid way, compare with the shift leader phone.

0929hrs I noticed that the magnet LHe level warning is flashing as low at 3600. The tell number for the cryogenic

picquet is 79640 rather than 70463. Level is "0" since Jan 2019 except for 3 'blips"

Kiosk technical shifter password is "Cms-Safety12345". see details in "Guidelines for CMS shifters" page 8.

Handed over to HCAL colleague so I can do the Safety Tour at 1138hrs. back at 1235. Removed the card BUT only put it back at 1319hrs.

Finally got the list of colleagues underground.TKS to all.